{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["TC Formatter","Read me","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TC Formatter","index":0,"n_rows":8,"n_cols":10,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
["Name","Description","Type","Value",null,null,null,null,"Thermal Coupling List File: ","D:\\users\\Test.txt"]
["TC-Hotbox-2","3.5mm bolts, small stiff surface 2.37 C/W x2","Total Conductance"," 1.68776371308017 W/°C"]
["Regulator-PCB","Perfect contact","Total Conductance"," 1000 W/°C"]
["Regulator-PCB-2","Perfect contact","Total Conductance"," 1000 W/°C"]
["Regulator-PCB-3","Perfect contact","Total Conductance"," 1000 W/°C"]
["Regulator-PCB-4","Perfect contact","Total Conductance"," 1000 W/°C"]
["GapPad","GapPad","Conductive Gap","1 W/(m*K)"]
["PCDU-PCB-HeatSink","3.5mm bolts 2.37C/W","Total Conductance"," 1.687 W/°C"]

{"sheet":"Read me","index":1,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["How to use:\n1. In NX select all the thermal couplings you wish to list.\n2. Right Click and select information\n3. In information window, select File Save As.. And save the contents to a text file\n4. Put full path of text file from 3. into cell K1\n5. Click 'Read File' button\n\nThermal couplings and key parameters are loaded into spreadsheet."]

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}